           20-07-99 June 1999 - ATLAS Week

    Electrode Spacer Test Program

                                                                         (The 1000 Tube Test= KTT)

·
            Module-0 Experience

                                                                     first insertion rate

             - FCAL1 nylon fibre:     1% shorts

             - FCAL2 PEEK clips:  20% shorts

                  repaired before beam test to

               FCAL1 = 1/2000

               FCAL2 = 20/2200

·
            Goal of KTT

                                                  - 1 short in 1000 on first insertion  = 0.1%

·
         Tested solution

                                                  - Improved tube cleaning (residual Cu flakes)

             - PEEK fibre spacer    (clips scraped Cu from

            tube walls)