       20-07-99 June 1999 - ATLAS Week

                                      Module Description & Setup

¯  FCal1  > 3/16 full module, Cu, 2350 electrodes

   Mechanical Performance:

       Channel Uniformity

       -                                   : ~ 1.5% uniformity

       H.V. performance  - 1 short during running

Electrode  spacer was soft

nylon fibre.

pf

                                                              C

                                                                         air

5

                                                                                                          232

±

                                                                                             =

    ¯  FCal2  > 1/4 full module, W/Cu, 2550 electrodes

        Mechanical Performance:

              Channel Uniformity

                                              -                                     :  ~ 1.5% uniformity

               H.V. performance  - 1% electrode shorts

                                studies show that this is due

    to PEEK insertion in copper

    tubes. Alternative under

    development.

pf

                                                         C

                                                                    air

3

6

                                                                                                   183

±

                                                                                        =
.