       20-07-99 June 1999 - ATLAS Week

                                          FCal1  Module-0 Construction

·

            Stacked drilled copper plates

·
       Copper tubes: I.D.  5.245 mm.

·
       Copper electrode rods: O.D. 4.712 mm.

                         - electrode gap  250
m

                         - 4 rods ganged at interconnect

.

·
       Designed spacer - kapton  coated quartz.

                         - breakage during installation

                         - Nylon used

·
       Copper tubes swaged in endplate.

                                              FCal2  Module-0 Construction

    ·

                Cu endplate - sintered tungsten matrix

    ·
            Copper tubes: I.D.  5.68 mm.

    ·
            Tungsten electrode rods: O.D. 4.93 mm.

                             - electrode gap  375
m

                             - 6 rods ganged at interconnect

.

    ·
            Designed spacer -  3 thermoformed PEEK

                                         clip spacers.

    ·
            Copper tubes swaged in endplate

.