24 bit x 16 FIFO

FIFO

24 bit x 16

reads out 8 TMCs

Each FMUX

1 TMC

0 TMC

To CIC

IN

Inp Control

Inp Control

IN

FMUX

FMUX

FMUX

FMUX

FMUX 0

1

2

3

4 3 bit serial lines to CIC

FMUX Architecture

Ownership

Slow Control

Data Controler

FETX